OR_LNLG_ESU

Description: |
This table contains Electro Surgery Units information for the surgical log (ORL).

Primary Key

Column Name | Ordinal Position |
--- | --- | ---
RECORD_ID | 1 |

Column Information

| Name | Type | Discontinued? |
--- | --- | --- | --- | ---
1 | RECORD_ID | VARCHAR | No |
The unique ID of the line record.
2 | ELECT_SURG_DEV_ID_PROV_NAME | VARCHAR | No |
The name of the service provider. This item may be hidden in a public view of the CLARITY_SER table.
3 | ELCT_SRG_MOD_TYP_C_NAME | VARCHAR | No |
The ESU device mode type.
May contain organization-specific values: Yes
Category Entries:
Monopolar
Bipolar
4 | ELECT_SURG_LOC_C_NAME | VARCHAR | No |
The location at which the ESU was applied.
May contain organization-specific values: Yes
5 | ELECT_SURG_LATER_C_NAME | VARCHAR | No |
The laterality of the location.
May contain organization-specific values: Yes
Category Entries:
Left
Right
Bilateral
N/A
Default
Unspecified
6 | ESD_TYPE_C_NAME | VARCHAR | No |
The ESU device type.
May contain organization-specific values: Yes
7 | ELECT_SURG_COAG_SE | NUMERIC | No |
The ESU coagulation settings.
8 | ELECT_SURG_CUT_SET | NUMERIC | No |
The ESU cut settings.
9 | ELECT_SURG_BSET_C_NAME | VARCHAR | No |
Stores the blend settings for the Electro Surgery Device.
May contain organization-specific values: Yes
No Entries Defined
10 | ELECT_SURG_COAG_HGH | NUMERIC | No |
Documents the high coagulation setting of a particular electrosurgical device.
11 | ELECT_SURG_CUT_HIGH | NUMERIC | No |
Documents the high cut setting of a particular electrosurgical device.
12 | ELECT_SURG_GPAPP_ID_PROV_NAME | VARCHAR | No |
The name of the service provider. This item may be hidden in a public view of the CLARITY_SER table.
13 | ELECT_SURG_PAD_LOT | VARCHAR | No |
Documents the lot number of the ESU's grounding pad.
14 | GROUND_PAD_EXP_DT | DATETIME | No |
This item stores the expiration date for an ESU grounding pad.
15 | BIPOLAR_SETTING | NUMERIC | No |
This item stores the bipolar setting for an Electro Surgery Device. This is the voltage.
16 | MONO_CUT_SETTING_C_NAME | VARCHAR | No |
The monopolar cut setting category number for the electro surgery unit.
May contain organization-specific values: Yes
No Entries Defined
17 | MONO_COAG_SETTING_C_NAME | VARCHAR | No |
The monopolar coagulation setting category number for the electro surgery unit.
May contain organization-specific values: Yes
No Entries Defined
18 | ESU_COAG_WATTAGE | INTEGER | No |
Stores information about the wattage for the coagulation setting of the electro surgery unit.
19 | ESU_CUT_WATTAGE | INTEGER | No |
Stores information about the wattage for the cut setting of the electro surgery unit.
20 | ESU_BIPOLAR_WATTAG | INTEGER | No |
Stores information about the wattage for the bipolar setting of the electro surgery unit.
21 | LIGASURE_ONE_LOW_C_NAME | VARCHAR | No |
The category number for the Ligasure 1 Low item. This is usually the same as the internal ID. If you use IntraConnect, this is the Community ID (CID).
May contain organization-specific values: Yes
No Entries Defined
22 | LIGASURE_ONE_HIGH_C_NAME | VARCHAR | No |
The category number for the Ligasure 1 High item. This is usually the same as the internal ID. If you use IntraConnect, this is the Community ID (CID).
May contain organization-specific values: Yes
No Entries Defined
23 | LIGASURE_TWO_LOW_C_NAME | VARCHAR | No |
The category number for the Ligasure 2 Low item. This is usually the same as the internal ID. If you use IntraConnect, this is the Community ID (CID).
May contain organization-specific values: Yes
No Entries Defined
24 | LIGASURE_TWO_HIGH_C_NAME | VARCHAR | No |
The category number for the Ligasure 2 High item. This is usually the same as the internal ID. If you use IntraConnect, this is the Community ID (CID).
May contain organization-specific values: Yes
No Entries Defined
25 | BIPOLAR_COAG_LOW | INTEGER | No |
The low bipolar coagulation setting for the electro surgery unit.
26 | BIPOLAR_COAG_HIGH | INTEGER | No |
The high bipolar coagulation setting for the electro surgery unit (ESU).
27 | BIPOLAR_SETTINGS_C_NAME | VARCHAR | No |
The category number for the Bipolar Output Settings item.
May contain organization-specific values: Yes
No Entries Defined
28 | GROUND_PAD_SER_NUM | VARCHAR | No |
This item stores the serial number of the ESU grounding pad.
29 | ELECT_SURG_PRESET_C_NAME | VARCHAR | No |
Store settings for ESU device.
May contain organization-specific values: Yes
No Entries Defined
30 | ESU_GAS_FLOW_HIGH | NUMERIC | No |
The high gas flow rate for the electro surgery unit.
31 | ESU_GAS_FLOW_LOW | NUMERIC | No |
The low gas flow rate for the electro surgery unit.
32 | ESU_COAG_SETTING | NUMERIC | No |
Item to document medium setting of ESU machines.
33 | ESU_CUT_SETTING | NUMERIC | No |
Item to document medium cut setting of ESU machines.
34 | ESU_MODULATION | INTEGER | No |
This item stores the numerical modulation setting for Electro Surgical Equipment.
35 | ESU_BIPOLAR_CUT_LOW | NUMERIC | No |
Documents the low cut setting of a bipolar electrosurgical device.
36 | ESU_BIPOLAR_CUT_HI | NUMERIC | No |
Documents the high cut setting of a bipolar electrosurgical device.